## @file
# A simple DXE_DRIVER that causes the PCI Bus UEFI_DRIVER to allocate 64-bit
# MMIO BARs above 4 GB, regardless of option ROM availability (as long as a CSM
# is not present), conserving 32-bit MMIO aperture for 32-bit BARs.
#
# Copyright (C) 2016, Red Hat, Inc.
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
##

[Defines]
  INF_VERSION                    = 0x00010005
  BASE_NAME                      = IncompatiblePciDeviceSupportDxe
  FILE_GUID                      = F6697AC4-A776-4EE1-B643-1FEFF2B615BB
  MODULE_TYPE                    = DXE_DRIVER
  VERSION_STRING                 = 1.0
  ENTRY_POINT                    = DriverInitialize

[Sources]
  IncompatiblePciDeviceSupport.c

[Packages]
  MdePkg/MdePkg.dec
  QemuQ35Pkg/QemuQ35Pkg.dec

[LibraryClasses]
  DebugLib
  MemoryAllocationLib
  PcdLib
  UefiBootServicesTableLib
  UefiDriverEntryPoint

[Protocols]
  gEfiIncompatiblePciDeviceSupportProtocolGuid ## SOMETIMES_PRODUCES
  gEfiLegacyBiosProtocolGuid                   ## NOTIFY

[Pcd]
  gUefiQemuQ35PkgTokenSpaceGuid.PcdPciMmio64Size                ## CONSUMES

[Depex]
  TRUE
