## @file
# A DXE_DRIVER providing SMRAM access by producing EFI_SMM_ACCESS2_PROTOCOL.
#
# Q35 TSEG is expected to have been verified and set up by the SmmAccessPei
# driver.
#
# Copyright (C) 2013, 2015, Red Hat, Inc.
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
##

[Defines]
  INF_VERSION                    = 0x00010005
  BASE_NAME                      = SmmAccess2Dxe
  FILE_GUID                      = AC95AD3D-4366-44BF-9A62-E4B29D7A2206
  MODULE_TYPE                    = DXE_DRIVER
  VERSION_STRING                 = 1.0
  PI_SPECIFICATION_VERSION       = 0x00010400
  ENTRY_POINT                    = SmmAccess2DxeEntryPoint

#
# The following information is for reference only and not required by the build tools.
#
#  VALID_ARCHITECTURES           = IA32 X64
#

[Sources]
  SmmAccess2Dxe.c
  SmramInternal.c
  SmramInternal.h

[Packages]
  MdeModulePkg/MdeModulePkg.dec
  MdePkg/MdePkg.dec
  QemuPkg/QemuPkg.dec
  QemuQ35Pkg/QemuQ35Pkg.dec

[LibraryClasses]
  DebugLib
  PcdLib
  PciLib
  UefiBootServicesTableLib
  UefiDriverEntryPoint

[Protocols]
  gEfiSmmAccess2ProtocolGuid   ## PRODUCES

[FeaturePcd]
  gQemuPkgTokenSpaceGuid.PcdSmmSmramRequire

[Pcd]
  gUefiQemuQ35PkgTokenSpaceGuid.PcdQ35SmramAtDefaultSmbase
  gUefiQemuQ35PkgTokenSpaceGuid.PcdQ35TsegMbytes

[Depex]
  TRUE
