/** @file
*  Debug Port Table (DBG2)
*
*  Copyright (c) 2020 Linaro Ltd. All rights reserved.
*
*  SPDX-License-Identifier: BSD-2-Clause-Patent
*
**/
#include <IndustryStandard/Acpi.h>
#include <IndustryStandard/DebugPort2Table.h>
#include <IndustryStandard/SbsaQemuAcpi.h>
#include <Library/AcpiLib.h>
#include <Library/PcdLib.h>

#pragma pack(1)

#define SBSAQEMU_UART_STR { '\\', '_', 'S', 'B', '.', 'C', 'O', 'M', '0', 0x00 }

typedef struct {
  EFI_ACPI_DBG2_DEBUG_DEVICE_INFORMATION_STRUCT Dbg2Device;
  EFI_ACPI_6_3_GENERIC_ADDRESS_STRUCTURE        BaseAddressRegister;
  UINT32                                        AddressSize;
  UINT8                                         NameSpaceString[10];
} DBG2_DEBUG_DEVICE_INFORMATION;

typedef struct {
  EFI_ACPI_DEBUG_PORT_2_DESCRIPTION_TABLE       Description;
  DBG2_DEBUG_DEVICE_INFORMATION                 Dbg2DeviceInfo;
} DBG2_TABLE;


STATIC DBG2_TABLE Dbg2 = {
  {
    SBSAQEMU_ACPI_HEADER (
      EFI_ACPI_6_3_DEBUG_PORT_2_TABLE_SIGNATURE,
      DBG2_TABLE,
      EFI_ACPI_DBG2_DEBUG_DEVICE_INFORMATION_STRUCT_REVISION
    ),
    OFFSET_OF (DBG2_TABLE, Dbg2DeviceInfo),
    1                                      /* NumberOfDebugPorts */
  },
  {
    {
      EFI_ACPI_DBG2_DEBUG_DEVICE_INFORMATION_STRUCT_REVISION,
      sizeof (DBG2_DEBUG_DEVICE_INFORMATION),
      1,                                   /* NumberofGenericAddressRegisters */
      10,                                  /* NameSpaceStringLength */
      OFFSET_OF (DBG2_DEBUG_DEVICE_INFORMATION, NameSpaceString),
      0,                                   /* OemDataLength */
      0,                                   /* OemDataOffset */
      EFI_ACPI_DBG2_PORT_TYPE_SERIAL,
      EFI_ACPI_DBG2_PORT_SUBTYPE_SERIAL_ARM_PL011_UART,
      {EFI_ACPI_RESERVED_BYTE, EFI_ACPI_RESERVED_BYTE},
      OFFSET_OF (DBG2_DEBUG_DEVICE_INFORMATION, BaseAddressRegister),
      OFFSET_OF (DBG2_DEBUG_DEVICE_INFORMATION, AddressSize)
    },
    ARM_GAS32 (FixedPcdGet32(PcdSerialRegisterBase)),  /* BaseAddressRegister */
    0x1000,                                            /* AddressSize */
    SBSAQEMU_UART_STR,                                 /* NameSpaceString */
  }
};

#pragma pack()

// Reference the table being generated to prevent the optimizer from removing
// the data structure from the executable
VOID* CONST ReferenceAcpiTable = &Dbg2;
