# Networking backends

The networking backend system connects guest-facing NICs (frontends)
to host-side packet I/O (backends) through a shared trait interface
defined in the `net_backend` crate. This page explains how the
pieces fit together, how packets flow, and how to navigate the code.

## Architecture overview

```text
┌──────────────┐  ┌──────────────┐  ┌──────────────┐
│ virtio_net   │  │   netvsp     │  │  gdma/bnic   │
│ (frontend)   │  │ (frontend)   │  │ (frontend)   │
└───────┬──────┘  └───────┬──────┘  └───────┬──────┘
        │                 │                 │
        │  &mut dyn BufferAccess            │
        │  (owned by frontend)              │
        │                 │                 │
        ▼                 ▼                 ▼
┌──────────────────────────────────────────────────┐
│  dyn Queue  (per-queue)                          │
│  poll_ready · rx_avail · rx_poll                 │
│  tx_avail · tx_poll                              │
└──────────────────────────────────────────────────┘
        ▲                 ▲                 ▲
        │                 │                 │
┌───────┴──────┐  ┌───────┴──────┐  ┌───────┴──────┐
│ TapQueue     │  │ConsommeQueue │  │  ManaQueue   │
│ DioQueue     │  │LoopbackQueue │  │ (hardware)   │
│   ...        │  │  NullQueue   │  │              │
└──────────────┘  └──────────────┘  └──────────────┘
```

There are three layers:

- **Frontend** — the guest-visible NIC device (`virtio_net`,
  `netvsp`, or `gdma`). Owns the `BufferAccess` implementation
  (no `Arc` or `Mutex` needed — each queue is driven from a single
  async task), translates between the guest-specific descriptor
  format and the generic `Queue` interface, and drives the poll
  loop.

- **Queue** — a single TX/RX data path created by the backend.
  Frontends interact with it entirely through the
  [`Queue`](https://openvmm.dev/rustdoc/net_backend/trait.Queue.html)
  trait. A device may have multiple queues for RSS.

- **Endpoint** — a backend factory. One per NIC. The frontend calls
  [`Endpoint::get_queues`](https://openvmm.dev/rustdoc/net_backend/trait.Endpoint.html#tymethod.get_queues)
  when the guest activates the NIC and
  [`Endpoint::stop`](https://openvmm.dev/rustdoc/net_backend/trait.Endpoint.html#tymethod.stop)
  on teardown.

See the
[`net_backend` rustdoc](https://openvmm.dev/rustdoc/net_backend/)
for the full trait signatures and type definitions.

## Packet flow

### Transmit (guest → host)

1. The guest posts a TX descriptor (e.g. a virtio descriptor chain
   or a VMBus RNDIS message).
2. The frontend reads the descriptor from guest memory, extracts any
   offload metadata (checksum, TSO, USO), and builds a `TxSegment` array.
   Each segment carries a guest physical address and a length — **no
   data is copied** at this point.
3. The frontend calls `queue.tx_avail(&mut pool, &segments)`. The
   backend reads data directly from guest memory via
   `pool.guest_memory()` and transmits it (e.g. writes to a TAP fd,
   posts to hardware, or feeds it to a user-space TCP stack).
4. If the backend completes synchronously (`tx_avail` returns
   `sync = true`), the frontend can immediately mark the descriptor
   done. Otherwise, it polls `tx_poll` later for async completions.

### Receive (host → guest)

1. The frontend pre-populates the backend with receive buffers by
   calling `queue.rx_avail(&mut pool, &buffer_ids)`.
2. When `queue.poll_ready(cx, &mut pool)` signals readiness, the
   backend has received a packet. It writes the packet data into
   guest memory through `pool.write_packet(rx_id, metadata, data)`.
3. The frontend calls `queue.rx_poll(&mut pool, &mut ids)` to
   collect the IDs of completed buffers, then delivers them to the
   guest (e.g. by completing virtio descriptors or sending VMBus
   completion packets).
4. The guest eventually returns the buffer, and the frontend recycles
   it via `rx_avail`.

### Guest memory access

The `Queue` interface works with guest physical addresses rather
than host buffers, giving each backend flexibility in how it
accesses packet data. The patterns fall into three categories:

**GPA pass-through (hardware DMA).** `net_mana` converts guest
physical addresses into IO virtual addresses (`GuestMemory::iova`)
and posts them as scatter-gather entries directly to GDMA hardware.
The NIC DMAs packet data to/from guest memory without any host-side
copy. This is the fastest path, but requires IOMMU mappings and
contiguous-enough buffers; when those conditions aren't met, MANA
falls back to bounce buffers.

**Host-mediated copy.** Software backends like `net_consomme` and
`net_dio` read TX data from guest memory with
`GuestMemory::read_at`, process or forward it, and write RX data
back with `BufferAccess::write_packet`. The data passes through
host memory, but the `Queue` interface avoids any extra copies
between the frontend and backend layers — the backend reads/writes
guest RAM directly.

## Lifecycle

1. The frontend creates a
   [`BufferAccess`](https://openvmm.dev/rustdoc/net_backend/trait.BufferAccess.html)
   implementation and one `QueueConfig` per queue.
2. It calls `endpoint.get_queues(configs, rss, &mut queues)`.
3. It enters the poll loop: `poll_ready` → `rx_avail` / `rx_poll` /
   `tx_avail` / `tx_poll`.
4. On shutdown, it drops the queues and calls `endpoint.stop()`.

## Backends

| Backend | Crate | Transport | Platform |
|---------|-------|-----------|----------|
| TAP | `net_tap` | Linux TAP device | Linux |
| DirectIO | `net_dio` | Windows vmswitch | Windows |
| Consomme | `net_consomme` | User-space TCP/IP stack | Any |
| MANA | `net_mana` | Azure hardware NIC (MANA/GDMA) | Linux |
| Loopback | `net_backend` | Reflects TX → RX | Any |
| Null | `net_backend` | Drops everything | Any |

## Frontends

| Frontend | Crate | Guest interface |
|----------|-------|-----------------|
| virtio-net | `virtio_net` | Virtio network device |
| netvsp | `netvsp` | VMBus synthetic NIC |
| GDMA/BNIC | `gdma` | MANA Basic NIC (emulated GDMA) |

## Wrappers

Wrappers implement `Endpoint` by delegating to an inner endpoint,
adding cross-cutting behavior:

- **PacketCapture** (`net_packet_capture`) — intercepts `rx_poll`
  and `tx_avail` to write PCAP-format packet traces. The capture
  path reads packet data from guest memory via `BufferAccess` and
  writes enhanced packet blocks to a ring buffer. Capture can be
  toggled at runtime; when disabled, the wrapper adds only an atomic
  load per call.

- **Disconnectable** (`net_backend`) — supports hot-plug and
  hot-unplug by swapping the inner endpoint at runtime.

## RSS and multi-queue

When a frontend supports Receive Side Scaling (RSS), it passes
multiple `QueueConfig` entries and an `RssConfig` (hash key +
indirection table) to `get_queues`. The backend creates one `Queue`
per entry and uses the RSS configuration to steer incoming packets
to the appropriate queue. Each queue is driven independently by its
own async task.

Currently `netvsp` and `net_mana` support multi-queue; `virtio_net`
is limited to a single queue pair.
